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Original nature of spill point.                                                            Installed 2’’flange with pipe connection @ 12 o;clock
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                                          repair in progress                                                               Spill point after repairs    
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