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Pix showing point bubbling before excavation  	      point exposed to see course of spill during jiv.
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Point prepared for patch welding.		         Point patch welded during jiv.
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[bookmark: _GoBack]Point after repair.			  	          Pix after Backfilling the repaired point. 
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