ZD,
Report of Joint Investigation Visit to 10’’ Diebu Creek-Nun River Delivery Line (D/L) , Bayelsa  State

A  . Attendance
1. Aroh  K. N------------------------------------------NOSDRA
2. Atiogoba Belema--------------------------------DPR
3. Adike Israel----------------------------------------BYSMEnv.
4. Dike Stanley---------------------------------------HSE-SPDC
5. Gerard E. Onuigho------------------------------Oil Spill Response-SPDC
6. Leo Uzogor----------------------------------------Geomatisc-SPDC
7. Iboro    I.         -----------------------------------Media-SPDS
8. Timi Zighadina (Chief)-------------------------Oporoma Community rep
9. Obikaboma Zighadina------------------------Oporoma Community rep
B. Spill Details: 
i. Location-10’’ Diebu Creek-Nun River D/L 
ii. Facility-SPDC
i. Spill Ref. No:1221605A
ii. Date of Spill-28/07/14
iii. Date Reported -28/07/14
iv. Date of JIV-04/08/14
v. Cause of Spill –Third party interference (illegal bunkering theft point )
vi. Spill co-ordinates-N040 48’ 00.6’’, E0060 06’ 28.9’’
vii. Quantity of spill- 5bbls
viii. Area of impact-1600m2

 Introduction: Following a report of crude oil spill in the above location, a JIV was carried out on August 4,, 2014 with the team in A above. 

2. Observation: The following observations were noted during the investigation.
 
i. Trenches and bund walls seen around the suspected leak point are indications of previous excavation.
ii.  Crude oil stained vegetation was  noticeable around the suspected leak point
iii. Upon manual exposure, a 4’’ metal valve installed  at 12 O’clock position  was seen on the flowline (see arrow) (fig.1)
iv. Repairs on the facility could not be concluded as at the end of  investigation
v. [image: C:\Users\KENNETH\AppData\Local\Microsoft\Windows\Temporary Internet Files\Content.Word\Photo1185.jpg]The spill incident was as a result of sabotage





 (
Fig. 1: 4’’ metal valve installed at 12 O’clock position on the Delivery Line 
)3. Recommendation:
SPDC should :
i. Ensure timely conclusion of  repairs on the facility to protect the environment 
ii. Strengthen surveillance network around its facility.
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