PHOTO STORY FROM POKO GARAGE EVENT RESPONSE OPERATION 2017 (GPS COORDINATE: N06 27 31.8 E003 21 58.7 {INCIDENT POINT})
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FIG 1: EVACUATION OF SAND FROM THE INCIDENT POINT (JAN. – FEB. 2017)
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FIG 2: EXCAVATED PIT WITH A MIXTURE OF PRODUCT AND WATER (FEB. 2017)
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FIG 3: SAFETY EQUIPMENT AND PROPERLY KITTED WORKERS (FEB. 2017)
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FIG 4: SOAKED ABSORBENT AT THE DRAINAGE AND RECOVERY TANK  (FEB. – MARCH 2017)
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FIG 5: CROSS SECTION OF TACKED PIPE JOINTS (APRIL 2017)
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FIG 6: PREPARATION FOR WELDING OF PIPE (APRIL 2017)
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FIG 7: WELDING IN PROGRESS (APRIL 2017)
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FIG 8: EXPOSED SECTION FOR INTEGRITY TEST (APRIL 2017)       
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[bookmark: _GoBack]FIG 9: PRESSURE TESTING GAUGE FOR THE REPAIRED PIPE  (MAY 2017)
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