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130mm Hack Saw cut on the 4” flow line        The absorbent booms put in place for containment
@ 6-11 0’clock position.                                      to avoid further spread of the spill.
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                                                     Repaired facility by the respond team
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