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REPORT OF JOINT INVESTIGATION VISIT (JIV) TO SHELL PETROLEUM DEVELOPMENT COMPANY (SPDC) 14” OKORDIA-RUMUEKPE (TRUNKLINE) PIPELINE @ UKPELIEDE, AHOADA WEST LOCAL GOVERNMENT AREA, RIVERS STATE.

Please find below highlights of JIV to the above location:
1. Company Address: The Shell Petroleum Development Company of Nigeria Limited, Shell Industrial Area, Rumuobiakani, P.O. Box 263, Port Harcourt, Rivers State.
2. Site/ Location: 14” Okordia-Rumuekpe (Trunkline) Pipeline @ Ukpeliede, Ahoada West Local Government Area, Rivers state.
3. Coordinates/ Incident Number: N 050  5’ 31.0 E 0060 31’ 44.6” / FED 2676375
4. Date of Incident: 29/06/2020.
5. Inspection Date and Time: 01/07/2020./ 14:00 HRS.
6. Inspection Team: 1) NWAORIE HUMPHREY			NOSDRA
    2) OGBULU, GP. IJEIJE			               RSMEnv
       7.    Site Contacts: 	   1) OKHUESE OHIS			               SPDC (OSR)
			   2) NANYO TELLY				SPDC (AHSS)
			   3) OTUZA CHIDOM		                             UKPELIEDE  COM. REP.
8.   Purpose of Inspection/ Investigation: It was a Joint Investigation Visit to investigate a reported incident by SPDC.  
9. Compliance History: Laws and Regulations of the Agency are complied with and the incident was promptly reported	
10. Opening Conference:  On arrival, toolbox meeting and safety briefing was conducted and the likely hazards of the job were enumerated. The Assets Holder Site Supervisor (AHSS) SPDC Mr. Nanyo Telly  told the JIV Team that the pipeline at the incident point runs from Okordia manifold to Rumuekpe manifold at about 32km. He also said that major maintenance activities were carried out on the pipeline and thereafter test running of the pipeline was done(flushing of the pipeline with water).
      11. Walk through Inspection: In the course of walk through inspection, the JIT observed;
I. The incident point was seen flooded.
II. Upon excavation of the incident point, a 3” nipple without a ball valve supported with a casted concrete was seen installed on the pipeline at 12 o’clock position by unknown persons for theft purpose.
III.  Water was seen gushing from the leak point 
     
12. Closing Conference: Immediately after JIV, the team departed from the oil spill site at about 4:45pm while repairs were on- going.
   13.   Compliance Concern: Not applicable.
   14.   Record of Inspection: NOSDRA JIV Forms and SPDC JIV Forms were duly signed and collected.
   15.   Sample Collected: Not applicable.
   16.   Photographs: 

		Spill Environment			Spill Points after excavation
      
        
17.   Recommendation:
· There is need for increase surveillance and security to discourage pipeline vandals and bunkerers.

18.   Signature and Date:
	Nwaorie, Humphrey.
	
SES.


