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REPORT OF JOINT INVESTIGATION VISIT (JIV) BY NOSDRA, RIVERS STATE MINISTRY OF ENVIRONMENT, HEIRS ENERGIES AND COMMUNITY MEMBERS TO 8’’ NKALI – IMO RIVER AT UMUOKECHI, ETCHE LGA, RIVERS STATE.
Please find below highlights of JIV to the above location.
COMPANY ADDRESS: Heirs Energies LTD, 71B Elelenwo Street, New GRA, Port Harcourt, Rivers State.
1. LOCATION/SITE ADDRESS: 8’’ NKALI – IMO RIVER AT UMUOKECHI COMMUNITY, ETCHE LGA, RIVERS STATE.
2. GEOREFERENCE COORDINATES/INCIDENT NUMBER:
N04 059’2.98’’, E007 007’ 31.16’’/ IN - 0663
3. DATE OF INCIDENT: 12/01/2024.
4. DATE OF REPORT: 12/01/2024.
5. INSPECTION DATE AND TIME: 12/01/2024 AT 1357HRS 
6. INSPECTION TEAM:
· NOSDRA		APEH, MALACHY I.
· RSMENV		ATTENG, CLAUDE C.
7. SITE CONTACTS:
· NPDC			 AYATSE, TERRY	  	
· COMMUNITY REP 	ISAIAH CHIDI
8. PURPOSE OF INSPECTION/ INVESTIGATION: Joint Investigation Visit (Event Response).
9. COMPLIANCE HISTORY: The site complies with the Agency’s law and regulations and HEIRS ENERGIES responded appropriately.
10. IMPACTED AREA: 264m2	
11. QUANTITY SPILLED:   40 Barrels
12. QUANTITY RECOVERED; 38 Barrels
13. OPENING CONFERENCE: After the initial welcome formalities, a tool-box/safety briefing coordinated by Mr Ayatse Terry (HEIRS ENERGIES Team Lead) was carried-out. Safety procedures required for the site work was explained to the JIT. The team members were also briefed about the oil spill incident.
10. WALK THROUGH INSPECTION       
During the walk-through inspection of the incident site, the following were observed:
· The Joint Investigation Team (JIT) on arrival observed a long trench along the company’s Right of Way.
· A section of the trench was found to be filled to half with Crude Oil suspected to have spilled from the facility.
· 5mm drilled hole was found on the facility at 4 O’clock position which was the sources of spill.
· At the time of JIV crude oil was still spilling from the vandalized section of the facility.
· The incident was as a result of Third-party interference (theft).
· Photographs of the incident point was taken during the JIV 
· The JIV was concluded successfully.
14. CLOSING CONFERENCE: At the end of the inspection, stakeholders signed off the JIV documents before departure from the site.
15. COMPLIANCE CONCERN:
· HEIRS ENERGIES has poor response equipment to oil spill incident
16. PHOTOGRAPHS:
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                         Figure 1&2: The 5mm Drilled Hole at 4 O’clock position and the impacted area.

17. RECOMMENDATION       
       It is recommended that:
· The company should increase surveillance around their facility to prevent similar incident in future.
     

       APEH, MALACHY I.
       PES.
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