PICTURES TAKEN AT THE JIV TO NAOC, EGBEGORO 11T FLOWLINE AT OMOKU COMMUNITY, ONELGA, RIVERS STATE.
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The spill point was covered with rag after the flowline was shut-in. The area around the spill point was heavily impacted. River boom was used to contain the spill from further spread.
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           A 80mm hacksaw cut on the line      
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