FH,
A REPORT OF JOINT INVESTIGATION VISIT TO OANDO ENERGY RESOURCES LIMITED FACILITY AT 14” OGBOINBIRI/TEBIDABA PIPELINE AT OLUGBOBORO, SILGA BAYELSA STATE ON 9TH DECEMBER, 2024.
            Please find below the highlights of the JIV to the above location.
1. Company Address: Oando Energy Resources Limited, Mile 4, Ikwere Road, P.O. Box 923. Port Harcourt, Rivers State, Nigeria.
Location/Site Address: 14” Ogboinbiri/Tebidaba Pipeline at Olugboboro, SILGA Bayelsa State.
2. Incident Number: 2024/SAR/252
3. Pollutant Type:    Crude oil
4. Quantity spilled:  10 bbls
5. Area of impact:    15928.66M2 
6. Quantity Recovered: Nil 
7. Coordinates: N040 36’ 52.8” E0050 57’ 01.9”     
8. Date of Incident: December 9th, 2024
9. Date first reported: December 9th, 2024
10. Inspection Date and Time: December 9th, 2024, 14:33hrs
11. Inspection Team: 
· EZEAMAECHI, EJIOFOR     NOSDRA
· SINGAR, IRO		           BYSMENV
12. Site Contact:
· GABRIEL MOSES	           OANDO HSE 
· BENSON OGBE                     OANDO CRV 
· ISAAC SIMON                    SURVEYOR     
13. Purpose of Inspection/Investigation: Event response.
14. Compliance History: OANDO complied by reporting incidents within 24hrs as mandated in the Agency’s Regulation.  
15. Opening Conference: Toolbox meeting was held at the muster point (on top 
of the barge) and the risks associated with the work and safety measures were highlighted including vital information about the spill incident. 
16. Walk through Inspection: 
 During the walk-through inspection of the incident site, the following were   observed:
I. The Joint Investigation Team (JIT) on arrival observed visible impact of oil on the surface.
II. The suspected incident point was exposed with the aid of swamp buggy on the company’s ROW.
III. The JIV team observed that vandals installed 3” valve at 12 o’ clock position of the pipeline for possible crude oil theft activity and the repair was conducted immediately 
IV. Based on the above observations, the JIT concluded that the incident was third party interference. 
V. JIV was successfully concluded.
17. Closing Conference: Signing of relevant JIV forms among all stakeholders 
	(NOSDRA, BYSMENV. and COMPANY REPS.) were done in the field.
18. Compliance Concerns: No compliance concern.
19. Record of Inspection:   
           NOSDRA form (JIV form)     
           Company form (OANDO form)
                Personnel Report
20. Photography: The pictures below are visual evidence captured during the JIV.    
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      Fig. 1: The state of the Environment at the time of JIV. Fig. 2: 3” valve installed at 12 o’ clock position
      21. Recommendations:	
I. OANDO should clean up the crude oil impacted area immediately.
		

This is submitted for your consideration and further directive, please

 
21        22. Signature and date:
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